BRONCO STANDARD FEATURES

Merhow’s Bronco Series trailers provide a significant list of standard features for this economical choice. You may select from straight load or slant load in both bumper pull and gooseneck configurations.

• Warranty 8 Year Structural
• Height 7’6” Width: 7’0”
• Stall Size Width at Sidewall: 40”, Diagonal Stall Length: 10’2”
• Short Wall 4’ - GN
• Chassis Tubular Aluminum with Tongue and Groove Extruded Aluminum Floor
• Dividers Alum. Formed Tubular Dividers w/ Hands Free Slam Latches, Padded, Spring Loaded
• Rear Tack Collapsible Wall, Removable Saddle Tree, Blanket Bars, Brush Box, Bridle Hooks, and Light
• Roof One Piece Aluminum, Cast Aluminum Corner Caps with Horse Logo
• Roof Bows Tubular Aluminum
• Rear Hoop Tubular Aluminum
• Rear Doors (2) Full Height Step-In Rear Doors, 20x20 Sliding Window w/ Screen and Bar Guards in Horse Door, Independent Two-Point Cam Latches.
• All Locks are Keyed Alike
• Escape Door Full Height and Width on Front of First Stall – on 3 Horse and Larger Units
• Axles Dexter Torsion Axles & Radial Tires
• Spare Tire Spare Tire and Wheel

• Brakes Electric Self Adjusting on all Wheels
• Coupler 2-5/16 Bulldog Top Latch – BP, Slide Latch - GN
• Jack Side Crank Moved to Rear of A-Frame - BP
• Single Leg - GN
• Skin White Baked-On-Enamel Aluminum fastened with 3M Tape
• Front Rock Guard on all Bumper Pulls
• Stall Area Walls Ballistic lined and insulated up 48" - .100 aluminum kick wall on hip side of Slant Loads
• Rubber Mats
• (1) Two-way pop up roof vents per stall
• Extruded aluminum DDFD each stall (slant loads)
• Hip windows with screen and bar guard
• (2) Exterior and interior horse ties per stall
• Electrical One L.E.D. Light per Horse Stall w/ Remote Switch
• All Exterior L.E.D. Lights
• LED Load Light
• Sealed Beam Flush Mount LED Tail Lights
• Dressing Room Rubber on floor
• Dome Light with Remote Switch
• 30x74 Dressing Room Door
• Drip Guard Above Dressing Room Door
• 2nd Location for Saddle Tree